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Fiber Media converter


  The non-managed media converters, which give you economic solutions for media conversion between fiber and copper Ethernet. It provides you SC, FC or ST connectors for your fiber optic cables and RJ45 for twisted pair UTP cable connection. The maximum extension is up to 40km over fiber. 
Features                                                         
* Data-rate of 1.25Gbps operation 

* In conformity to IEEE 802.3, IEEE802.3ab 1000 base-T, 1000 base-FX, IEEE802.3z, 1000base-SX/LX, IEEE802.1a, IEEE802.1PQ0S, IEEE802.1d Spanning Tree.

* +3.3V single power supply.

* Hot Pluggable & Wall-Mountable.
* Stable performance more than 50 thousand hours with fault-free.        

* Unique IC solution applied.
* Supports 10/100/1000M full/half duplex, easy upgrades.
* Auto MDI/MDI-X.

* Auto-negotiation & speed autosensing
* Support flow control.
* Concentrated into EF16-D220(16slot for media converter cards) or EF14-D220(14slot for media converter standalone type) 2U rack-mount chassis.
* In conformity with Compliant with SFP MSA and SFF-8472. 

* Stable performance more than 50 thousands hours with fault-free.
* In conformity with safety code of FCC, CE and RoHS.

Specifications

	Optical Interface
	Connector
	SC/UPC (1000Base FX) 

	
	Data Rate
	1000Mbps

	
	Mode
	Full duplex

	
	Fiber
	SM 9/125um

	
	Distance
	10/100/1000Mbps:

SM 40km

	
	Wavelength
	SM 1310nm (Tx/Rx)

	UTP Interface
	Connector
	1 Port Ethernet 10/100/1000 Base-TX (RJ45)

	
	Data Rate
	10/100/1000Mbps

	
	Mode
	Half/full duplex

	
	Cable
	Cat5, Cat6

	Power Input
	Adapter Type
	DC5V(default), 12V/48V(Optional)

	
	Power Built-in Type
	220VAC ± 10%, 50/60 Hz switching type

	Power Consumption
	＜3W

	Weight
	Adapter Type
	0.39kg

	
	Power Built-in Type
	0.67kg

	Dimensions
	Adapter Type
	94*70.5*26.5cm

	
	Power Built-in Type
	140.5*111*30cm

	Temperature
	0~55℃ Operating; -40~70℃ Storage

	Humidity
	5~95%RH (no condensing)

	MTBF
	≥ 10.0000h

	Certification
	CE,FCC,RoHS


Application
* Extend your Ethernet connection up to 0~120km away using fiber optics

* Creates an economical Ethernet-fiber/copper-fiber link for connecting remote sub-networks to larger fiber optic networks/backbones

* Converts Ethernet to fiber, fiber to copper/Ethernet, ensuring optimum network scalability for connecting two or more Ethernet network nodes (e.g. connecting two buildings on the same campus)

* Designed to provide high-speed bandwidth for demanding large scale work groups that require expansion of Gigabit Ethernet Network
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Product Pictures

	10/100M Dual Fiber
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	10/100M Single Fiber
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	10/100/1000M Dual Fiber
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	10/100/1000M Single Fiber
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System Design

1. For Networking
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2. For CCTV Surveillance Security
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Order Information

	Part Number
	Rate
	Optic fiber
	Wavelength

(nm)
	Power

(dBm)
	Rx sensitivity

(dBm)
	Reach

(KM)

	BT-950GS-40
	10/100/1000Mbps
	SM
	1310
	-5~3
	-25
	40
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